**CITY OF BILOXI**

**SPECIAL PROVISION NO. 907-321-1 CODE: (SP)**

**DATE: 06/15/2017**

**SECTION 321 - IN-GRADE PREPARATION**

# Subsection 321.03.6 - Density

Delete Subsection 321.03.6 in its entirety and insert the following paragraph:

The required density for in-grade preparation of all courses shall equal or exceed 95% density in accordance with ASTM D 1557.