**CITY OF BILOXI**

**SPECIAL PROVISION NO. 907-403-1**

**DATE: 06/26/2017**

**SECTION 403: ASPHALT PAVEMENTS**

**907-403.03.2 – Smoothness Tolerances.**

Delete the final three paragraphs of this subsection.

**907-403.03.2.1 – Smoothness Tolerances for Mean Roughness Index (MRI).**

Delete the last sentence of the eleventh paragraph, “No unit price adjustment will be applied on any underlying lift.”

After the eleventh paragraph, delete the remaining paragraphs associated with this subsection and add the following paragraph:

For Category A and B projects, when the long continuous interval MRI exceeds 20 inches per mile more than that allowed for the particular type project, the surface lift shall be removed and replaced. For Category C projects, when the long continuous interval MRI for the final surface does not show more than a 30% improvement over the existing surface profile and has a final surface MRI greater than 100 inches per mile, the surface lift shall be removed and replaced.

**907-403.05 – Basis of Payment.**

In the first sentence of the first paragraph, delete reference to 403.03.2.