**CITY OF BILOXI**

**SPECIAL PROVISION NO. 907-501-1 CODE: (IS)**

**DATE: 06/26/2017**

**SECTION 501: CONCRETE PAVEMENTS**

**907-501.03.19 – Surface Test.**

Delete the first sentence of paragraph eleven and replace with the following:

Corrections shall be made using an approved profiling device. In the event the MRI exceeds that allowed for the Category of project by 20 inches per mile, the segment in question shall be removed and replaced.

**907-501.05.3 – Price Adjustments for Smoothness.**

Delete this subsection in toto.