**CITY OF BILOXI**

**SPECIAL PROVISION NO. 907-627-1 CODE: (IS)**

**DATE: 07/03/2017**

**SECTION 627 – RAISED PAVEMENT MARKERS**

**Subsection 627.03.2 – Construction Details:**

Insert the following paragraph after the last paragraph of Subsection 627.03.2.

Two-Way Blue Reflective Raised Markers shall be placed in the center of the lane nearest to and directly perpendicular from each fire hydrant, unless otherwise directed by the City Engineer or his Authorized Representative.